Note: Must ground FTDI cable too! (AKA: HAve a common ground between power supply and arduino, or else bad data transmission)

Normally, RX -> TX.

On the Arduino, RX -> RX